-----------------------------------------------------------------------------
Package Version                 2.6.0
-----------------------------------------------------------------------------

Platform                        evo_g8_cxp (Standard allPIXAevo 8K CoaXPress)

Bitstream version:              12.2.0
Application version:            6.6.0
Camera descr. (xml) version:    6.6.0
Feature Reference:              6.6.0
Boot file version:              6.1.0

-----------------------------------------------------------------------------
Files
-----------------------------------------------------------------------------

- allPIXAevo_application_g8_cxp_6.6.0.bin
- allPIXAevo_bitstream_g8_cxp_12.2.0.bin
- allPIXAevo_bootfile_g8_cxp_6.1.0.bin
- allPIXAevo_gamma_general_lut_KaxGamma03_10.dd
- allPIXAevo_listfile_g8_cxp_2_6_0-rst.ini
- allPIXAevo_listfile_g8_cxp_2_6_0.ini
- allPIXAevo_packagedescriptionfile_g8_cxp_2_6_0.ini
- allPIXAevo_xml_g8_cxp_6.6.0.bin
- allPIXAevo_xml_g8_cxp_6.6.0.xml
- features_reference_6.6.0.pdf

-----------------------------------------------------------------------------
Note
-----------------------------------------------------------------------------

-> The bootfile version 6.x.x requires at least firmware 6.6.0-beta.2 for proper operation.


Changes and new Features
------------------------

-> Internal refactoring
-> Improvement of the internal voltage control

-> Monitor the g8 training state at runtime
-> Support multiple PRNU data sets for the LED-Flashing Mode(Up to two)
-> Changed the visibility of DeviceVersion, DeviceManufacturerInfo features from Invisible to Beginner
-> Improvement in gain control
-> Improvement in  black level control
-> Added the DeviceLogLevel feature
-> FlatFieldCorrection
	-> Added new features for flat field correction to replace the older features
	   -> FlatFieldCorrectionSelector
	   -> FlatFieldCorrectionEnable
	   -> FlatFieldCorrectionDataSetdescription
	   -> FlatFieldCorrectionDisplayReference
	   -> FlatFieldCorrectionAvaialblePlanes
	   -> FlatFieldCorrectionFirstPixel
	   -> FlatFieldCorrectionLastPixel
	   -> FlatFieldCorrectionStartCalibration
	   -> FlatFieldCorrectionStopCalibration
	   -> FlatFieldCorrectionCalibrationStatus
    -> Added IsDeprected for few fetaures in ImageCalibrationControl category
    -> Changing either old or new features will update the other feature accordingly
    -> All the deprecated features still can be used but from version 3.0.0 it will be removed completely.
	
-> Log can be accessed by LogFile in FileAccessControl

Bug Fixes
------------------------
-> Fixed bug in checking the line time for min when setting it
-> Fix the bug of an extra frame when using the FrameActiveExtendLines
-> Fix in led flash out lines(5-8) which were modified while loading user set
-> Fixed bug of sometimes xml url string was wrong and leading to "Discovery Failure" when trying to retrieve the xml
-> Fixed a bug in setting the exposure Time
-> Fixed for getting the maximum exposure time, it was limited to RGB and IR, but neglecting the White filter.(Releated to Individual exposure)
-> Update Min Line Period, to a valid value before, changing the exposure time at the sensor to avoid invalid states
-> Fixed disabling FFC-Data-Set bug. (Could not disable wrong data set)
-> Removed "Unsigned" from 64-bit InReg node in XML, because it is not supported by GenAPI
-> Adapted to get more valid min line time for TDI mode
-> Fix for 3 or 4 cxp channel streaming 
-> The related bug to less number of lines in TDI mode is removed
-> Fix for sensor pgood and traning errors
-> Manage overflow by too high darkref pixels

Incompatibilities
------------------------


Errata
------------------------


-> LED-Flashing-Control:
	- Problems are expected when Frame Trigger and Line Trigger are off.
	- Errors are expected when exceeding the minimum sequence time

-> The Internal DSNU/PRNU creation may not work properly. Please check the result is good or not.

-> In Master Slave Mode there may be a constant shift between the cameras

-> There may be issues with Gamma

-> The CXP source tag in the streaming protocol is not reliable


