
# Version 7.0.0
Standard allPIXAevo 32K CoaXPress
## Component Versions
|      Variant      |         Version         |
|   ------------    |      -------------      |
| Bitstream         |          23.0.0         |
| Application/XML   |          14.1.0         |
| Bootfile          |          16.0.0         |
| Feature Reference |          14.1.0         |
| Gamma    	        |      KaxGamma03_10      |


## Notes




## Changes and new Features


* Use new sensor configuration to extend reset level.
  * Achieving 90,9KHz line rate


## Bug Fixes




## Incompatibilities


* Due to new sensor configuration it is recommended to recreate the DSNU/PRNU


## Errata


* The Internal DSNU/PRNU creation may not work properly. Please check the result is good or not.
* In Master Slave Mode there may be a constant shift between the cameras
* The gain control is not working when gain control region is outside the ROI
* Led flash may not work properly
  * With some settings camera does not deliver any images
  * With some other settings there can be one pattern missing


## Docs

